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	S. No.
	Parameter
	Existing SEPA Standards
	Proposed SEQS (Sindh EPA)

	01
	Sulphur Dioxide (SO2)
	Annual= 80ug/m3
24hrs= 120ug/m3
	Annual= 50ug/m3
24hrs= 80ug/m3

	02
	NO
	Annual= 40ug/m3
24hrs= 40ug/m3
	Annual= 40ug/m3
24hrs= 40ug/m3

	03
	NO2
	Annual= 40ug/m3
24hrs= 80ug/m3
	Annual= 40ug/m3
24hrs= 80ug/m3

	04
	O3
	1 hr= 130ug/m3
	1 hr = 130ug/m3

	05
	Suspended Particulate Matters (SPM)
	Annual= 360ug/m3
24hrs= 500ug/m3
	Annual= 360ug/m3
24hrs= 500ug/m3

	06
	Lead (Pb)
	Annual= 1ug/m3
24hrs= 1.5 ug/m3
	Annual= 0.5 ug/m3
24hrs = 1ug/m3

	07
	Carbon
	8 hr= 5mg/m3
	8 hr = 5mg/m3

	08
	Carbon Monoxide (CO)
	1 hr= 10mg/m3
	1 hr = 10mg/m3

	09
	PM10
	Annual= 120ug/m3
24hrs= 150ug/m3
	Annual= 60 ug/m3
24hrs= 100ug/m3

	10
	PM2.5
	Annual= 40 ug/m3
24hrs= 75 ug/m3
	 Annual= 15 ug/m3
 24hrs = 35 ug/m3
 1hrs = 15 ug/m3












	Existing & Proposed Sindh Environmental Quality Standards for Industrial Gaseous Emission (mg/Nm3)

	S. No.
	Parameter
	Existing SEPA Standards
	Proposed SEQS (Sindh EPA)

	01
	Smoke
	40% or 2 Ringleman Scale or equivalent smoke number 
	40% or 2 Ringleman Scale or equivalent smoke number 

	02
	PM
	100
	10-120 mg/Nm3

	03
	Sulphur Oxides 
	1700 mg/Nm3
	200-400 mg/Nm3 (Coal-fired power plant )
10-20 mg/Nm3 (Gas-fired power plant)
300-500 mg/Nm3(Lignite-fired power plant )

	04
	Carbon Monoxide (CO)
	800 mg/Nm3
	100-200 mg/Nm3

	05
	Lead
	50 mg/Nm3
	0.5-1 mg/Nm3

	06
	Mercury
	10 mg/Nm3
	0.03-0.1 mg/Nm3

	07
	Cadmium
	20 mg/Nm3
	0.1-0.2 mg/Nm3

	08
	Arsenic
	20 mg/Nm3
	0.1-0.2 mg/Nm3

	09
	Copper
	50 mg/Nm3
	0.5-1 mg/Nm3

	10
	Antimony
	20 mg/Nm3
	20 mg/Nm3

	11
	Zinc
	200 mg/Nm3
	1-2 mg/Nm3

	12
	Oxides of Nitrogen 
	1200 mg/Nm3 (Coal-fired power plant )
400 mg/Nm3 (Gas-fired power plant)
600 mg/Nm3(Oil-fired power plant )
	300-600 mg/Nm3 (Coal-fired power plant )
50-100 mg/Nm3 (Gas-fired power plant)
400-700 mg/Nm3(Lignite-fired power plant )





	Existing & Proposed Sindh Environmental Quality Standards for Municipal and Liquid Industrial Effluents (mg/L)

	S. No.
	Parameter
	Existing SEPA Standards
	Proposed SEQS (Sindh EPA)

	01
	Biological Oxygen Demand (BOD) at 20˚C
	80
	60

	02
	Chemical Oxygen Demand (COD)
	150
	150

	03
	Total Suspended Solids (TSS)
	200
	150

	04
	Total Dissolved Solids (TDS)
	3500
	2100

	05
	Temperature 40˚ or Temperature Increase
	<3˚C
	<3˚C

	06
	pH Value
	6 - 9
	6 - 9

	07
	Oil and Grease
	10
	10

	08
	Phenolic Compounds (as phenol)
	0.1
	1

	09
	Chloride (as CL-)
	1000
	1000

	10
	Fluoride (as F-)
	10
	10

	11
	Cyanide (as CN-) total
	1
	0.2

	12
	An-ionic detergents (as MBAS) (2)
	20
	20

	13
	Sulphate (SO₄²¯)
	600
	600

	14
	Sulphide (S²¯)
	1
	1

	15
	Ammonia (NH₃)
	40
	40

	16
	Pesticides
	0.15
	0.15

	17
	Cadmium
	0.1
	0.1

	18
	Chromium (trivalent and hexavalent) 
	1
	0.5

	19
	Copper
	1
	1

	20
	Lead
	0.5
	0.1

	21
	Mercury
	0.01
	0.01

	22
	Salenium
	0.5
	0.05

	23
	Nickle
	1
	1

	24
	Silver
	1
	0.5

	25
	Total Toxic Metals
	2
	Undesirable

	26
	Zinc
	5
	5

	27
	Arsenic
	1
	0.5

	28
	Barium
	1.5
	1.5

	29
	Iron
	8
	3.0

	30
	Manganese
	1.5
	1.5

	31
	Boron
	6
	2.0

	32
	Chlorine
	1
	1



